Airbus A320

**Before start up**

Thrust levers Idle

Engine Master Switch OFF

Engine mode selector Normal

Parking brake SET

Landing gear lever Down

Windshield wipers OFF

**Start up**

Bateries ON

APU fire test Check both lights

APU Master switch ON

APU Start

Set Lights

Displays ON

ADR ON

Seatbells ON

Emergency exit lights ON

APU bleed ON

Fuel pumps Automatic

Engine 1 fire test Done

Engine 2 fire test Done

Public Address

Warning light test Done

Anti Skid ON

Radios Check

Weather radar OFF

Lower ECAM display Check

Thrust levers Idle

Engine Master Switch OFF

Engine mode selector Normal

Ground spoilers Retracted and disarmed

Flaps UP

Trim Zero

Parking brake SET

Gravity gear extension Correct position

Transponder SET

MCD a FMGC SET

QNH SET

Navigation display Set NAV

Autopilot SET

Clearance ASK

Beacon light ON

Engine mode selector START

Engine 2 Master Switch ON

Wait to engine spool up

Engine 1 Master Switch ON

Wait to engine spool up

After start up - Engine mode selector NORM

**Taxi**

Flight controls CHECK

FLT instrument CHECK

T.O. speeds / FLX. temp CHG/REV

Taxi lights ON

**Before take off**

Cabin report RECIEVED

ATC/TCAS/FCU SET

PACKS AS REQUIED

ECAM TO MEMO CHECK NO BLUE LINE

Landing lights ON

Flaps Set for take off (8)

Ground spoilers ARM

T.O. Check CHECK

**After take off**

Baro ref SET

LDG Gear UP

Flaps RETRACTED

PACKS ON

**Approach**

Briefing CONFIRMED

ECAM status CHECK

Seat bells ON

BARO REF SET BOTH

**Landing (At or below 1500ft AGL)**

Cabin report RECIEVED

A/THR Speed / OFF

ECAM / LDG MEMO CHECK NO BLUE LINE

**After Landing**

Spoilers DISARMED

Flaps As RQRD

WX Radar / PWS OFF / OFF

TCAS SBY

APU START